| Trilobite 1.4 User Guide | © Darwin Arts L.L.C., 2016

# Smoother Module

This module acts as an extreme low pass filter smoothing function for signals routed into port 0, with the input to port 1 acting to control the degree of low-pass smoothing. This module is ideal for adding control-rate change of audio modules, with a good use case being to add portamento to pitch changes from the value sequencer or midi input module.

For a key to understanding the tables on this page, see the Module Types page.

## Adding Input Ports

Adding input ports is not enabled for this module.

## Static Parameters

  # | Title | Type | Description
  0 | Center Mix Pos | Multiple Choice | Has the options: Balanced at half, which causes the smoother to use control port inputs in the range [0,1], ideal for parameter control of smoothing. Balanced at zero, which causes the smoother to use control port inputs in the range [-1, 1], ideal for when the smoothing control signal is an LFO.

## Input Ports

  # | Title | Description | Input Scalar Used | Parameter Scalar Used
  0 | Input Signal | Input signal source. | NO | NO
  1 | Smoothing Factor | The degree to which the input signal is smoothed (low-pass filtered) in the output signal. Accepts input in the range [0, 1] or [-1,1] depending on the Center Mix Pos static parameter value. Higher values will produce a smoother output signal. | YES | YES

## Output Ports

  # | Title | Description
  0 | Smoother Signal | A low-pass filtered version of the input signal.