| Trilobite 1.4 User Guide | © Darwin Arts L.L.C., 2016

# Gate Module

This module acts as a counter-balanced mixer for two input signals with the mix balance controlled by a third signal. If only one input signal is routed into the module, it acts as a basic gate modulator.

For a key to understanding the tables on this page, see the Module Types page.

| The Gate Module is available in Pro Version only.

## Adding Input Ports

Adding input ports is not enabled for this module.

## Static Parameters

  # | Title | Type | Description
  0 | Center Mix Pos | Multiple Choice | Has the options: Balanced at half, which causes the gate to proportionately mix A/B signals from input ports using a mix range of [0, 1] with 0.5 being the position at which input port scaling is equal.. Balanced at zero, which causes the gate to proportionately mix A/B signals from input ports using a mix range of [-1, 1] with 0.0 being the position at which input port scaling is equal..

## Input Ports

  # | Title | Description | Input Scalar Used | Parameter Scalar Used
  0 | Signal A | Input signal source. | NO | NO
  1 | Signal B | Input signal source. | NO | NO
  2 | A/B Mix Balance | Control signal which sets the mix ratio of Input Source B to Input Source A. | YES | YES

## Output Ports

  # | Title | Description
  0 | Gate-mixed Signal | Either a synthesized vocal sound or filtered version of Glottal Source signal.