| Trilobite 1.4 User Guide | © Darwin Arts L.L.C., 2016

# Sample Hold Module

The Sample Hold Module, when triggered by a input signal on one port, then capture the instantaneous signal value on its other port and relay that value to the output port until triggered again. When transitioning between held values, the module provides a smoothing function to prevent sudden discontinuities in output

For a key to understanding the following tables, see the Module Types page.

| The Sample Hold module is available in Pro Version only.

## Adding Input Ports

Adding input ports is not enabled for this module.

## Static Parameters

None.

## Input Ports

  # | Title | Description | Input Scalar Used | Parameter Scalar Used
  0 | Capture Signal | Instantaneous values will be captured from the signal routed to this port when a trigger value is received on Port 1. | NO | NO
  1 | Hold Trigger | Trigger Signal. When input on this port rises above value 0.5, A trigger state is activated and the Capture Signal will be sampled for a value to be held and routed to output. | NO | NO

## Output Ports

  # | Title | Description
  0 | Hold Value | The sampled signal value, which changes only as fast as the module is triggered.