| Trilobite 1.4 User Guide | © Darwin Arts L.L.C., 2016

# Oscillator Module

The oscillator module creates an oscillating waveform of the indicated function type at the frequency specified by its input Control Signal. Available function types are sinusoidal, square, triangle, and sawtooth.

For a key to understanding the tables on this page, see the Module Types page.

## Adding Input Ports

Adding input ports is not enabled for this module.

## Static Parameters

  # | Title | Type | Description
  0 | Function Type | Choice | Has the options Sine Square Triangle Sawtooth
  1 | Phase | Floating-point | indicates the initial phase of the waveform as a ratio value. Range: [0, 1], LINEAR

## Input Ports

  # | Title | Description | Input Scalar Used | Parameter Scalar Used
  0 | Frequency Signal | The input signal to this port controls the module oscillation frequency in cycles per second (Hz) | YES | YES

## Output Ports

  # | Title | Description
  0 | Output Signal | The oscillating waveform. Range: [-1, 1]