| Trilobite 1.4 User Guide | © Darwin Arts L.L.C., 2016

# Pitch Tracker Module

The Pitch Tracker Module provides a rough continuous approximation of the peak frequency of its input signal in the form of an output signal, which reports the instantaneous frequency as a sliding Signal in Hz (cycles per second).

For a key to understanding the tables on this page, see the Module Types page.

## Adding Input Ports

Adding input ports is not enabled for this module.

## Static Parameters

None.

## Input Ports

  # | Title | Description | Input Scalar Used | Parameter Scalar Used
  0 | Input Signal | An audio signal to be analyzed. Connections from an Input Module work best. | NO | NO

## Output Ports

  # | Title | Description
  0 | Instant Pitch Value | This signal is an approximation of the real-time peak pitch value of the input signal, in Hz., but rendered as a continuous signal suitable for input to an Oscillator Module.