| Trilobite 1.4 User Guide | © Darwin Arts L.L.C., 2016

# Summation Module

The Summation Module adds together all connected input signals with scaling applied and produces a single output signal. In essence, it acts as a signal mixer, or mux.

For a key to understanding the tables on this page, see the Module Types page.

## Adding Input Ports

Adding input ports is enabled for this module, up to a limit of 16 inputs.

## Static Parameters

None.

## Input Ports

  # | Title | Description | Input Scalar Used | Parameter Scalar Used
  N | Mixer Input Signal #N | An input signal which will be mixed. | YES | YES

## Output Ports

  # | Title | Description
  0 | Mixed Output Signal | The mixed signal. Range: no range limit